**CABRI 605 PARTITION WALLS**
Doors, partition walls and front walls made of Cabrillant toughened safety glass (ESG) as per EN 12150-2. Float 10 mm, entire surface enamelled using screen printing process, all edges polished smooth. Colours as per standard colour range. Glass height     cm.

Doors, partition walls and front walls made of Cabrillant toughened safety glass (ESG) as per EN 12150-2. Listral SR 200, 10 mm, (textured surface), entire surface enamelled, all edges polished smooth. Colours as per standard colour range. Glass height     cm.

Doors, partition walls and front walls made of Cabrillant toughened safety glass (ESG) as per EN 12150-2. Satinato 10 mm (satin finish on one side), entire surface enamelled using screen printing process, all edges polished smooth. Colours as per standard colour range. Glass height     cm.

Doors, partition walls and front walls made of Cabrillant toughened safety glass (ESG) as per EN 12150-2. Float, bright white 10 mm (glass without green cast), entire surface enamelled using screen printing process, all edges polished smooth. Colours as per standard colour range. Glass height     cm.

Doors, partition walls and front walls in Cabrillant laminated safety glass (LSG), comprising 2x 5 mm Float toughened safety glass (ESG) as per EN 12150-2. 1 sheet of glass in centre enamelled over entire surface using screen printing process, 1.52 mm PVB film. Glass height     cm.

Doors open inwards.

Angle brackets used for wall fixing and connection of partition walls with front walls. No visible screw fittings.

Fixed front parts supported by partition wall feet on ready tiled floor. Floor rosette in solid aluminium. Ground clearance    cm.

Partition walls stabilised at top by continuous circular tube, recessed, diameter 25 mm.

Fittings

In each cubicle: 2 Aluminium alloy door hinges with stainless
 steel pin and nylon sliding surfaces, incl. integrated spring
 to hold the doors open
 1 Olive lock with internal
 knob and external red/green indicator
 1 Door bumper, theft-proof fitting
 1 Screen between
 door hinges on interior
 1 Screen on lock side,
 applied on interior

Alternative: 1 Lock with aluminium handle. External
 red-green indicator, internal rotary olive handle

 All fittings clear anodised, stainless

Construction parts:

All connecting elements in aluminium (DIN 1725) are 100% corrosion-resistant and environmentally friendly. 100% recyclable.

Enamelled safety glass:

Enamels are lead- and cadmium-free, 100% recyclable.