**CABRI 628 URINAL – MODESTY PANELS**  
In Cabrillant toughened safety glass (ESG) as per EN 12150-2. Float 10 mm, entire surface enamelled using screen printing process, all edges polished smooth. Colours as per standard colour range.  
Size 45 x 90 cm.  
  
Wall fixing of urinal modesty panel using two double angle brackets.  
No visible screw fittings.  
  
Construction parts:  
  
All connecting elements in aluminium (DIN 1725) are 100% corrosion-resistant and environmentally friendly. 100% recyclable.  
  
Enamelled safety glass:  
  
Enamels are lead- and cadmium-free, 100% recyclable.