**CABRI 601 PARTITION WALLS**  
Partition walls made of Cabrillant toughened safety glass (ESG) as per EN 12150-2. Float 10 mm, entire surface enamelled using screen printing process, all edges polished smooth. Colours as per standard colour range. Glass height     cm.  
  
Partition walls made of Cabrillant toughened safety glass (ESG) as per EN 12150-2. Listral SR200, 10 mm, (textured surface), entire surface enamelled, all edges polished smooth. Colours as per standard colour range. Glass height     cm.  
  
Partition walls made of Cabrillant toughened safety glass (ESG) as per EN 12150-2. Satinato 10 mm (satin finish on one side), entire surface enamelled using screen printing process, all edges polished smooth. Colours as per standard colour range. Glass height     cm.  
  
Partition walls made of Cabrillant toughened safety glass (ESG) as per EN 12150-2. Float, bright white 10 mm (glass without green cast), entire surface enamelled using screen printing process, all edges polished smooth. Colours as per standard colour range. Glass height     cm.  
  
Partition walls in Cabrillant laminated safety glass (LSG), comprising 2x 5 mm Float toughened safety glass (ESG) as per EN 12150-2. 1 sheet of glass in centre enamelled over entire surface using screen printing process, 1.52 mm PVB film. Glass height     cm.  
  
Partition walls fixed to wall with angle brackets.  
No visible screw fittings.  
  
Partition walls with partition wall feet stand on ready tiled floor. Floor rosette in solid aluminium.  
Ground clearance    cm.  
  
Partition walls stabilised at top by continuous circular tube, recessed, diameter 25 mm.  
  
All fittings in clear anodised aluminium, stainless  
  
Construction parts:  
  
All connecting elements in aluminium (DIN 1725) are 100% corrosion-resistant and environmentally friendly. 100% recyclable.  
  
Enamelled safety glass:  
  
Enamels are lead- and cadmium-free, 100% recyclable.