**PARTITION WALLS CABRI 905 floating with invisible fastening**

The partition feet and thestabilizing rod are relegated back-

and give the system a [flush](https://dict.leo.org/englisch-deutsch/flush)-mounted, elegant

and a floating impression.   
  
Fittings outside utilizing invisible point fastening.   
  
Doors, forehead and side walls made of Cabrillant composite safety  
glass 15 mm CSG made of 8 + 6 mm float extra-white single-pane  
safety glass (ESG)

according to EN 12150-2. Both glasses are enamelled in the middle full-surface,  
EVA film 0.8 mm, all edges polished flat.

Partition walls made of Cabrillant laminated safety glass LSG  
made of 2 x 5 mm float extra-white single-pane safety glass  
(ESG) according to EN 12150-2.   
Both glasses in the middle all-surface enamelled,  
EVA – foil 0.8 mm, all edges polished flat.   
  
Glass height     cm.   
  
Doors inward - opening.

Wall fastening and connection of the partition walls with the end walls

with cross-fitting and rosettes

including strengthening angle.

Partition wall with partition wall base supported on the

pre-tiled floor. Soil rosette in aluminium solid.

Ground clearance cm.

Stabilization of the partition walls utilizing a run-through,

recessed round tube, diameter 25 mm.   
  
Fittings

per cell: 2 Light metal door bands with Stainless steel axis of

rotation and Nylon sliding surfaces,

incl. built-in spring   
for holding a position of the doors

1 Olive lock with inner turn knob,  
 outside with red-green display

Housing and cover rosette in V4A  
 1 door buffer, theft-proof mounted

1 clamp screen protection between the door bands on the inside

1 View protection on the lock side inside

mounted.

**All fittings colourless anodised, stainless**  
construction parts:   
  
All fasteners in aluminium (DIN 1725) are 100%

corrosion-resistant and environmentally friendly.

100% recycling capability.   
  
Enamelled safety glass:  
  
enamel colours lead- and cadmium-free, 100%  
recycling possibility.