**PARTITION WALLS CABRI 905 room-high with invisible fastening**  
fittings outside using invisible point fastening.   
  
Doors, forehead and side walls made of Cabrillant composite safety  
glass 15 mm CSG made of 8 + 6 mm float extra-white single-pane  
safety glass (ESG) according to EN 12150-2.

Both glasses are enamelled full-surface,  
EVA film 0.8 mm, all edges polished flat.

Partition walls made of Cabrillant composite safety glass CSG  
made of 2 x 5 mm float extra-white tempered safety glass  
(TSG) according to EN 12150-2.   
Both glasses in the middle all-surface enamelled,  
EVA – foil 0.8 mm, all edges polished flat.   
  
Glass height     cm with a skylight over doors.   
  
Doors inward - opening.   
  
Connection of the partition walls with the end walls with

Cross fitting and rosettes including reinforcement angle.

Partition walls standing in aluminium U-profile (colourless anodized)

mounted, without ground clearance.

Fittings

per cell: 2 Light metal door bands with Stainless steel axis of rotation   
 and Nylon sliding surfaces,

incl. built-in spring   
for holding a position of the doors

1 Olive lock with inner turn knob,  
 outside with red-green display

Housing and cover rosette in V4A  
 1 door buffer, theft-proof mounted

1. clamp screen protection between

the door bands on the inside

1 View protection on the lock side inside

mounted.

**All fittings colourless anodised, stainless**

construction parts:

All fasteners in aluminium (DIN 1725) are 100% corrosion-resistant and environmentally friendly. 100% recycling capability.   
  
Enamelled safety glass:

enamelled colours lead- and cadmium-free, 100%  
recycling possibility.